|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | 21013 GALLARATE (VA) - ITALIA  Via Cappuccini, 50/A  VAT: 03190400121 | |  |  |  |  |  | | --- | --- | --- | --- | --- | | REQUEST DATE | | |  | | |  |  |  | |  |   Object: harness in mounting box |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| COMPANY: | | | | | | |
| QUANTITY (HARNESSES): | | | | | | |
| HOOKS\*1:  OUR PLASTIC HOOK ( )  STAUBLI RAPID ATTACK ( )  BONAS RAPID ATTACK ( )  NONE | | | | | | |
| CORD:  YES (QUANTITY PER HARNESS KG 1 COLOR  2 COLORS)  NO | | | | | | |
| COMBER BOARD: PLEASE COMPLETE THE FORM IN THE COMBER BOARD PAGE OF THE WEB SITE AND ATTACH IT TO THIS PAGE. | | | | | | |
| HEALD TYPE AND QUANTITY (R 1020, SR312 ECC): | | | | | | |
| SPRING: WEIGHT (GRAMS) : | | | LENGTH (MILLIMETERS): | | | |
| HEALD-SPRING: | COMPLETE ASSEMBLY | PARTIAL ASSEBLY | | | | NOT ASSEMBLED |
| JUNCTION TUBE:  1 COLOR | | | 2 COLORS | | | |
| GUIDING BOARD:  YES: SPECIFICATE JACQUARD TYPE AND MODEL | | | | | NO | |
| JACQUARD: MODEL: SIZE (HOOKS): | | | | | | |
| COMBER BOARDS FRAMES:  YES, CHOOSE MATERIAL AND LENGHT | | | | | NO | |
| PAINTED IRON  ALLUMINIUM LENGTH (CENTIMETERS): | | | | | | |
| SPRINGS FRAME:  YES, LENGTH (CENTIMETERS): | | | | NO | | |

\*1: FILL THE QUANTITY IN THE EMPTY SPACE ( HOOKS PER HARNESS)

ALL QUANTITY MUST BE FOR AN HARNESS